Node 1 Node 2

initial state x = 0, y = 0 1. write x, no fault 2. write y, page fault 3. send request to Node 1 4. send page to Node 2 5. receive page 6. write y, no fault final state x = 1, y = 1

Figure 10.16 Page fault handling in a DSM.

Copyright © 2000 by Addison Wesley Longman, Inc.